

**SALES ORDER REQUISITION & SUPPLY COLUMN**

ChemDist Process Solutions Pvt Ltd

# INDIA Address:

|  |  |
| --- | --- |
| QRN No. | **QRN:5294 R4** |
| Type. |  |
| Job No. | SO-652 |
| Date | 29/06/2022 |
| Rev | R0 |

Plot No J-174/1, J Block, PCNTDA, Bhosari, Pune-411026, Maharashtra Mobile: +91-9545500345

Email[: info@chemdist.in](mailto:info@chemdist.in)

1. **SCOPE OF SUPPLY :**


**Our scope of supply includes Manufacturing & Supply of below listed items:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Equipment** | **MOC** | **QTY** | **Manufacturing Sr No.** |
| **Reboiler** | **CS** | **1 No** | **CDPS-652-E1917-2022** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Sr No.** | **TAG Nos.** | **QTY** | **Description** |
| 1 | **FALLING FILM REBOILER (FFE)** | 1 No | Falling Film Reboiler for C-202A  **AREA- 125 m2 MOC**  Shell : SA516 Gr.70  Tube : SA 179  Tube OD - 38.1 mm  Tube Thk - 2.1\* mm  Tube Length - 6000 mm  No of Tubes – 174 Nos  Distributor with Tube Inserts  **Design Data**  Shell Side  Design Pressure : 6 kg/cm2 Design Temperature : 355 Deg C  Tube Side  Design Pressure : 10 kg/cm2 Design Temperature : 325 Deg C  Along with Nozzles, Flanges, Body Flanges, Tube sheets, Hardware & spiral wound gaskets |

## Notes:

1. All ‘\*’ mark shall be confirmed by design team.
2. All thicknesses shall be confirmed by design team.



|  |  |
| --- | --- |
| Delivery Date (FOR-Site) | **9th Sep 2022** |
| Internal Inspection Report | Required |
| TPI | YES |
| Remark/Instruction | Test Certificates Required as per QAP |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Signature** | | |
| Prepared By | PMD | | |
| Checked By | PMD |  |  |
| Approved By | TW | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Issued By** | **Signature** | **Received By** | **Signature** |
| Marketing |  | Design/Dwg |  |
|  |  | Manufacturing |  |
|  |  | Purchase |  |